 

**Specifications**

* **Operating Temperature: -13°F to 140°F (-25°C to 60°C)**
* **Power Supply: 1 x 9V battery**
* **Battery Life: 55 hours of intermittent use, with low-battery indicator**
* **Weight: 2 lbs. (0.9 kg)**
* **Dimensions: 34 inches overall length**
* **Submergibility: Water-resistant up to the handle grip (30 inches)**
* **Circuit Board: Surface mount technology with silicon-protected coating**

**Locating Depths:**

* **Survey Markers: Up to 9 feet**
* **PK Nails: Up to 1 foot**
* **Valve & Curb Boxes: Up to 10 feet**
* **Manhole Covers: Up to 10 feet**
* **Cast Iron Pipes: Up to 8 feet**
* **Septic Tank Handles: Up to 4 feet**
* **Steel Drums: 5 to 12 feet**
* **Oil Tanks: Up to 15 feet**
* **Well Casings: Up to 17 feet**
* **Road Culverts: Up to 10 feet**
* **Catch Basins: Up to 8 feet**
* **Fire Hydrants: Up to 4 feet**
* **Warranty:** 2-year limited warranty (terms and conditions may vary outside the U.S.)

 