**Operating Frequency of Search Coil:** 4.5 kHz

**Sensitivity Adjustment.** Range: 12:1

**Output Indication:** Meter - 1 milliamp, 1 - 100 linear scale

Speaker - 16 Ohm impedance

Headset (optional) - 8 Ohm impedance

**Audio Frequency:** 450 Hz

**Power Supply:**................. +/- 9 V, (2) 9V NEDA 1604

**Coil Configuration:** Double D

**Weight:** 2.8 lbs (1.3 kg)

**Dimensions:.....................** Control Box 3 x 5 x 6 inches (8 x 12 x 16 cm)

Handle 0.75 x 23 inches (1.9 x 58.4 cm)

**Shipping Weight:** 4 lbs (1.8 kg)

**Shipping Dimensions:** 26.5 x 6.25 x 6.25 inches (67 x 16 x 16 cm)