Search Loop Configuration Double D (direct wired)

Output Frequency of Loop 4.5kHz,

 Output Indication Speaker 16 ohm impedence

 Audio frequency 450 Hz

Power Supply 9V, each

Power Consumption (-9V) 17 mA

. (+9V) 4mA min, 6 mA sound

. threshold, 125 mA max sound

Weight with 8” coil .................. 4.25 lbs.

Operating Temp .. -4 0 to +1580F (-200 to +700C)

. search loop immersible in water

Dimensions Length 28” to 48” adjustable

. (71cm to 122 cm)

Shipping Weight 7 lbs.

Shipping Dimensions 34.75” x 12.75” x 5.25”

. (88.3 x 32.4 x 13.3cm)